Classful Addressing (Solved Question 1)

For usable addresses we subtract 2 because .0 is for network address and 255 is broadcast address.

