Stop and Wait ARQ (Automatic Repeat request) Protocol

1. After transmitting one frame the sender waits for an ack before transmitting the next frame.
2. If the ack does not arrive after a certain period of time, the sender times out and retransmits the original frame.
3. Stop and wait ARQ = Stop-and-wait + timeout timer + sequence number
4. Scenarios: 