Selective Repeat ARQ

1. It is a sliding windows protocol
2. Only the erroneous or lost frames are retransmitted, while correc rames are received and buffered.
3. The receiver while keeping track of sequence numbers, buffers the frames in memory and sends NACK for only frame which is missing or damaged
4. The sender will send/retransmit packet for which NACK is received.