Basic of IP Addressing

IP Address

1. IP stands for internet protocol
2. Every node in the computer network is identified with the help of an IP address.
3. Logical Address
4. Can change based on the location of the device
5. Assigned by manually or dynamically
6. Represented in decimal and it has 4 octets (x.x.x.x).
7. 0.0.0.0 to 255.255.255.255 (32 bits)

